**The BeatLove
The Beatles Tribute Show

Technical rider (ENG)**

**Vocals:**

1. Four cable mics (Shure Beta 58)
2. Two straight mic stands (Voc1 и Voc2), 2 boom mic stands (Voc3 и Voc4)
3. 220V outlet (Voc1)

**Drums:**

1. Professional drumset (Ludwig, Yamaha, Sonor, Tama or Pearl)

22” bass drum
12” rack tom
14” or 16” rack tom
2 cymbal stands
1 hi-hat stand
Snare drum with stand
Bass drum pedal
Drum throne
Professional cymbals set (hi-hat, crash, ride)

1. Drum mic kit (Shure, Sennheiser or Audix)
2. For a large concert hall drum riser is required (minimal size 2х2х0,5m)
3. No drum shield is allowed

**Bass guitar:**

1. Bass amp (Vox, Ampeg, Gallen-Krueger, Hartke or EBS)
2. DI-BOX
3. Jack-Jack cable
4. 2 guitar stands

**Guitars:**

1. Guitar amp (Vox AC30, Fender Twin Reverb or Deluxe) miked by Shure sm57 or Sennheiser e904, Jack-Jack cable
2. Guitar amp (Vox AC30, Fender Twin Reverb or Deluxe) miked by Shure sm57 or Sennheiser e904, Jack-Jack cable
3. 6 guitar stands
4. DI-BOX for Acoustic guitar

**Keys:**

1. Professional workstation or electric piano (Yamaha, Nord, Roland, Kurzweil)
2. Sustain pedal
3. 2 DI-BOX
4. 2 Jack-Jack cables
5. Keyboard stand
6. Throne
7. 220V outlet

**Playback:**

1. XLR-cable to drummer
2. 220V outlet

**Monitors:**

1. 3 in-ear body packs (Sennheiser or Shure)
2. Cable for drummer's in-ear (Jack-Jack)
3. 5 stage monitors 12”+1,5”

**Input list:**

|  |  |  |  |
| --- | --- | --- | --- |
| **CH** | **INSTRUMENT** | **MIC/DI-box** | **INSERT** |
| 1 | Kick  | Shure Beta 52A (Audix D6) | gate/compressor |
| 2 | Snare  | Shure SM 57A (Audix i5) |  |
| 3 | Hi-hat | Shure SM 81, AKG С 451 |  |
| 4 | Rack tom  | Sennheiser e904 (ShureBeta 98, 56) | gate/compressor |
| 5 | Floor tom | Sennheiser e904 (ShureBeta 98, 56) | gate/compressor |
| 6 | Overhead L | Shure SM 81, AKG С 451 |  |
| 7 | Overhead R | Shure SM 81, AKG С 451 |  |
| 8 | Play Back | XLR |  |
| 9 | Bass | Active Di-box | compressor |
| 10 | Guitar L | Shure SM 57, SENNHEISER E906 |  |
| 11 | Guitar R | Shure SM 57, SENNHEISER E906 |  |
| 13 | Keyboard 1 L | Di-box |  |
| 14 | Keyboard 2 R | Di-box |  |
| 15 | Voc1 | Shure Beta 58A | compressor |
| 16 | Voc2 | Shure Beta 58A | compressor |
| 17 | Voc3 | Shure Beta 58A | compressor |
| 18 | Voc4 | Shure Beta 58A | compressor |
| 18 | Acoustic Guitar | Di-box |  |

**Stage plan:**

****

*If you got any questions please mail me: sergey@beatlove.net*